Publication information

Geomatics Canada
Open File 7

Ground deformation produced by 2012 M6.4 and M6.3 Ahar double earthquakes mapped with RADARSAT-2 DInSAR

S.V. Samsonov and M. Czarnogorska

© Her Majesty the Queen in Right of Canada, as represented by the Minister of Natural Resources Canada, 2015

doi:10.4095/296205

Publications in this series have not been edited; they are released as submitted by the author.

View the licence agreement at http://data.gc.ca/eng/open-government-licence-canada

Recommended citation

Samsonov, S.V. and Czarnogorska M., 2015. Ground deformation produced by 2012 M6.4 and M6.3 Ahar double earthquakes mapped with RADARSAT-2 DInSAR; Geomatics Canada, Open File 7, 1 .zip file. doi:10.4095/296205

Contents

Open file contains information about ground deformation produced by 2012 M6.4 and M6.3 Ahar double earthquakes mapped with RADARSAT-2 DInSAR. We provide deformation maps in GMT format and supplementary information necessary for modeling.

Directory structure

Data folder names are in the following format SATELLITE-BEAM 
RADARSAT2_MF5
RADARSAT2_MF6

Description of files:

*.rmli.par.txt – parameter file of master image describing satellite, beam and processing parameters
*.adf.diff.png – map of wrapped filtered interferogram
*.adf.unw.png – map of unwrapped filtered interferogram
*adf.unw.geo.png and *adf.unw.geo.kml – Google Earth kml files (unwrapped interferogram re-wrapped for visualization)
*adf.unw.grd – GMT (the Generic Mapping Tool) grid file of unwrapped filtered interferogram (final product)
bperp.txt – file with interferogram baseline information

lv_theta.png – map of SAR look-vector elevation angle
lv_theta.grd – GMT grid file of SAR look-vector elevation angle

lv_phi.png – map of SAR look-vector orientation angle
lv_phi.grd – GMT grid file of SAR look-vector orientation angle

Adobe®, Acrobat®, and Reader® are either registered trademarks or trademarks of Adobe Systems Incorporated in the United States and/or other countries.

System requirements

PC with 486 or greater processor, or Mac® with OS® X v. 10.2.2 or later; Adobe® Reader® v. 6.0 or later; video resolution of 1280 x 1024.

Author contact information

S.V. Samsonov (sergey.samsonov@nrcan-rncan.gc.ca)
Canada Centre for Mapping and Earth Observation, Natural Resources Canada
560 Rochester, Ottawa, ON K1A0E4, Canada

Availability information

This publication is available for free download through GEOSCAN (http://geoscan.nrcan.gc.ca/).