Publication information

Geological Survey of Canada
Open File 7903

Structural and Depth Contours of the Lower-Middle Aldridge Contact, East Kootenay Region, Southeastern British Columbia

Eric A. de Kemp and Ernst M. Schetselaar

© Her Majesty the Queen in Right of Canada, as represented by the Minister of Natural Resources Canada, 2015

doi:10.4095/297429

Publications in this series have not been edited; they are released as submitted by the author.

View the licence agreement at http://data.gc.ca/eng/open-government-licence-canada

Recommended citation

de Kemp, E.A. and Schetselaar, E.M.,  2015. Structural and Depth Contours of the Lower-Middle Aldridge Contact, East Kootenay Region, Southeastern British Columbia; Geological Survey of Canada, Open File 7903, 
1 .zip file. doi:10.4095/297429

Contents

This Open File presents contoured 2D map representations of the Lower–Middle Aldridge Contact (LMC) as well as a 3D viewer to examine the regional geometry of the LMC. The outline of the Sullivan Pb,Zn,Ag depoit is included for reference on map and 3D views. 

3 PDF files in the Maps\ directory, OF7903_1.pdf, OF7903_2.pdf and OF7903_3.pdf can to be opened with Adobe® Acrobat Reader DC 2015 An installer is provided in Utils\ readerdc_en_ma_install.exe for viewing and plotting.
 
A free 3D viewer is provided with this data set from Leapfrog®. Copy the installer file either  Utils\ Viewer64Setup4.3.0.exe or Utils\ViewerSetup4.3.0.exe to your local machine and double click on it to set up the viewer on 32 bit or 64 bit PC systems. Once the leapfrog viewer is installed, double click on Maps\ LMC_2015.lfview for opening from the leapfrog file browser. 

Projection of all data is in Universal Trans Mercator (UTM) Zone 11, Horizontal Datum NAD 83, Vertical Datum NAD83, Horizontal and vertical map units in meters. Elevation Z values are positive upwards.   

A set of (25) faults the LMC horizon, LMC sub-surface and surface observation points and structural observations are included in the Export\ directory in DXF, Gocad and SHAPE file formats.  

See Notes section on the map sheets for source data, methodology and usage instructions.

Directory structure

.\
Readme.rtf

Exports\
	DXF\
Alki_fault.dxf
Arrow_fault.dxf
Boulder_Creek_fault.dxf
Carrol_Creek_fault.dxf
Dibble_fault.dxf
Faults_3D_Regional_Traces.dxf
Hall_Lake_fault.dxf
Kimberley_fault.dxf
LMC_2014_2K_contours.dxf
LMC_2014_Contours.dxf
LMC_2015.dxf
LMC_Depth_2015.dxf
LMC_Elevation_2015.dxf
LMC_Fault_Polygons.dxf
Lewis_Lower_fault.dxf
Mather_fault.dxf
Mathew_Creek_fault.dxf
Moyie_East_fault.dxf
Moyie_fault.dxf
NE_102_fault.dxf
NE_108_fault.dxf
NE_110_fault.dxf
NE_213_fault.dxf
NS_103_fault.dxf
NW_105_fault.dxf
Perry_Creek_fault.dxf
RMT_fault.dxf
Spyder_fault.dxf
St_Mary_fault.dxf
Sully_EW_fault.dxf
Sully_NW_fault.dxf

	Gocad\
Alki_fault.ts
Arrow_fault.ts
Boulder_Creek_fault.ts
Carrol_Creek_fault.ts
Dibble_fault.ts
Hall_Lake_fault.ts
Iron_Range_fault.ts
Kimberley_fault.ts
LMC.pl
LMC_2014.ts
LMC_2015.ts
LMC_3D.vs
LMC_3D_Dense.vs
LMC_DDH_2015.vs
LMC_Depth_2015.pl
LMC_Elevation_2015.pl
Lewis_Lower_fault.ts
Mather_fault.ts
Mathew_Creek_fault.ts
Moyie_East_fault.ts
Moyie_fault.ts
NE_102_fault.ts
NE_108_fault.ts
NE_110_fault.ts
NE_213_fault.ts
NS_103_fault.ts
NW_105_fault.ts
Perry_Creek_fault.ts
RMT_fault.ts
S0_2014.vs
Spyder_fault.ts
St_Mary_fault.ts
Sully_EW_fault.ts
Sully_NW_fault.ts

	Shape\
LMC_2015_Depth.shp
LMC_2015_Elevation.shp
LMC_DDH_XYZ.shp
S0_2015.shp
S1_2015.shp

Maps\ 
OF7903_1.pdf
OF7903_2.pdf
OF7903_3.pdf
LMC_2015.lfview
Utils\
	
readerdc_en_ma_install.exe
Viewer64Setup4.3.0.exe
ViewerSetup4.3.0.exe

Adobe®, Acrobat®, and Reader® are either registered trademarks or trademarks of Adobe Systems Incorporated in the United States and/or other countries.

ESRI®, ArcExplorer™ and ArcReader™ are trademarks, registered trademarks, or service marks of ESRI® in the United States, the European Community, or certain other jurisdictions.

Leapfrog® is a registered trademark of ARANZ Geo Limited 

Gocad® and SKUA® are registered trademarks of Paradigm Corporation

Digital Topographic Data from Natural Resources Canada and Province of British Columbia GeoBC (TRIM) 

System requirements

PC with 2 GHz or greater CPU processor, 32.0 GB RAM recomended, Windows 7 or greater (64 bit recommended), Adobe® Reader® v. 6.0 or later; video resolution of 1280 x 1024.

Author contact information

Eric A. de Kemp (eric.dekemp@canada.ca)
Geological Survey of Canada
Ottawa, Ontario, K1A 0E8

Availability information

This publication is available for free download through GEOSCAN (http://geoscan.nrcan.gc.ca/).